## This is guide to test Serial data reading using Arduino Uno via Wokwi

## Wiring

A circuit board with wires

Description automatically generated

## Code

void setup() {

  // put your setup code here, to run once:

**Serial**.begin(9600);

}

void loop() {

  // put your main code here, to run repeatedly:

  int sensorValue = analogRead(A0);

**Serial**.println(sensorValue);

  delay(1);

}